Appendix E

KBOGUS format

The KBOGUS file is used to replace specific observations in a station report. It is accessed by RAWINS as FORTRAN unit 12.

The KBOGUS record format is

40 FORMAT(I4, I2, 1X, A8, 1X, F7.1, 1X, F7.1, 4(1X, F7.1), 2X, I2, 4X, I8)

Each record describes corrections to be made to a single station at a single level. More than one variable may be modified by a KBOGUS record, if desired.

Following is an example of four records of a KBOGUS file. The titles and dashed lines are for clarification purposes only.

-------------------------------------------------------------------------------
N TY STA PRES HT TEMP RH DIR SPD L DATE
-------------------------------------------------------------------------------
1 2 72270 1 1019.7 88888.0 99999.9 88888.0 88888.0 88888.0 1 87010412
1 2 72564 1 88888.0 88888.0 88888.0 88888.0 50.0 3.6 1 87010412
1 2 ZFFC 1 88888.0 88888.0 16.0 88888.0 88888.0 88888.0 1 87010412
1 1 72220 1 88888.0 88888.0 88888.0 88888.0 195.0 37.0 4 87010412
-------------------------------------------------------------------------------

Description of KBOGUS file variables

N: Number of observations for the given date, variable and level.

TY: Type of level: 1: mandatory level 2: surface -1: nonmandatory level

STA: Five digit station identifier followed by a flag (1 or 2) indicating whether one or two surface observations from a single station (i.e., surface station report; surface observation from an upper-air station) were both used in a surface analysis.

PRES: Bogus sea-level pressure (mb) to insert. Two other options are available: to retain the original value, PRES = 88888.0; to delete the original value without inserting a bogus value, PRES = 99999.0.

HT: Bogus height (m). Again, options 88888.0 (to retain original value) and 99999.0 (to delete original value) may be used.

TEMP: Bogus temperature (ffiC). 88888.0 (retain); 99999.0 (delete).

RH: Bogus relative humidity (%). 88888.0 (retain); 99999.0 (delete).

DIR: Bogus wind direction (degrees). 88888.0 (retain); 99999.0 (delete). SPD: Bogus wind speed (m s�^1). 88888.0 (retain); 99999.0 (delete). L: Level: 1 = surface, 2 = 1000 mb, 3 = 850 mb, etc.; the highest values of L refer to nonmandatory levels.

DATE: Eight digit date/time identifier, in the format YYMMDDHH.